(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 53)
    (tracks 321)
    (zones 0)
    (modules 86)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 SYNC-OUT)
  (net 4 RIGHT)
  (net 5 SL)
  (net 6 S$33979)
  (net 7 LPF)
  (net 8 YM-LEFT)
  (net 9 YM-RIGHT)
  (net 10 SCD-RIGHT)
  (net 11 32X-RIGHT)
  (net 12 PSG)
  (net 13 32X-LEFT)
  (net 14 SCD-LEFT)
  (net 15 LEFT)
  (net 16 SYNC-75)
  (net 17 R-OUT)
  (net 18 G-OUT)
  (net 19 B-OUT)
  (net 20 R-IN)
  (net 21 G-IN)
  (net 22 B-IN)
  (net 23 SR)
  (net 24 "NET-(CON101-PAD6)")
  (net 25 "NET-(U101-PAD7)")
  (net 26 "NET-(U101-PAD8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net 32X-LEFT)
    (add_net 32X-RIGHT)
    (add_net B-IN)
    (add_net B-OUT)
    (add_net G-IN)
    (add_net G-OUT)
    (add_net GND)
    (add_net LEFT)
    (add_net LPF)
    (add_net "NET-(CON101-PAD6)")
    (add_net "NET-(U101-PAD7)")
    (add_net "NET-(U101-PAD8)")
    (add_net PSG)
    (add_net R-IN)
    (add_net R-OUT)
    (add_net RIGHT)
    (add_net S$33979)
    (add_net SCD-LEFT)
    (add_net SCD-RIGHT)
    (add_net SL)
    (add_net SR)
    (add_net SYNC-75)
    (add_net SYNC-OUT)
    (add_net YM-LEFT)
    (add_net YM-RIGHT)
  )
  (module easyeda:MD-90SM (layer F.Cu) (tedit 0)
    (at -873.341 -678.345)
    (fp_text reference CON1 (at 6.885 4.32) (layer B.SilkS))
    (fp_text value MD-90SM (at 4.902 7.874 180) (layer Cmts.User) hide)
    (fp_text user rep494 (at 0 0) (layer Cmts.User))
    (pad 5 thru_hole circle (at -0.127 2.794 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 3 SYNC-OUT))
    (pad 8 thru_hole circle (at -2.159 2.794 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 5 SL))
    (pad 9 thru_hole circle (at -4.191 2.794 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 23 SR))
    (pad 4 thru_hole circle (at 1.905 2.794 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 16 SYNC-75))
    (pad 7 thru_hole circle (at 3.937 2.794 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 17 R-OUT))
    (pad 3 thru_hole circle (at 3.937 0.254 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 18 G-OUT))
    (pad 6 thru_hole circle (at -4.191 0.254 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 24 "NET-(CON101-PAD6)"))
    (pad 1 thru_hole circle (at 1.143 0.254 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 19 B-OUT))
    (pad 2 thru_hole circle (at -0.889 0.254 180) (size 1.524 1.524) (drill oval 1.016 1.021) (layers *.Cu *.Paste *.Mask)
      (net 2 +5V))
    (pad 10 thru_hole circle (at -0.127 -3.302 180) (size 3.048 3.048) (drill oval 2.286 2.291) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at -7.366 -2.54 180) (size 3.048 3.048) (drill oval 2.286 2.291) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 7.112 -2.54 180) (size 3.048 3.048) (drill oval 2.286 2.291) (layers *.Cu *.Paste *.Mask)
      (net 1 GND))
  )
  (module easyeda:OSHW-LOGO_5MM (layer F.Cu) (tedit 0)
    (at -871.55 -654.685)
    (fp_text reference G (at -0.743 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at -0.293 0) (layer B.Fab) hide)
    (fp_text user gge124594 (at 0 0) (layer Cmts.User))
  )
  (module easyeda:DMP-8 (layer F.Cu) (tedit 0)
    (at -878.154 -665.81 270)
    (attr smd)
    (fp_text reference U3 (at -0.66 0.219 270) (layer F.SilkS))
    (fp_text value DMP-8 (at -0.381 -5.804 270) (layer F.Fab) hide)
    (fp_text user gge140421 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.905 3.051 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
    (pad 2 smd rect (at -0.635 3.051 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
    (pad 3 smd rect (at 0.633 3.048 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 S$33979))
    (pad 4 smd rect (at 1.905 3.051 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.907 -3.051 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 S$33979))
    (pad 6 smd rect (at 0.633 -3.05 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
    (pad 7 smd rect (at -0.637 -3.05 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
    (pad 8 smd rect (at -1.907 -3.05 270) (size 0.72 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
  )
  (module easyeda:JUMPER_PADSX3 (layer F.Cu) (tedit 0)
    (at -875.424 -648.627)
    (attr smd)
    (fp_text reference d (at 2.108 0.025) (layer F.SilkS))
    (fp_text value JUMPER_PADSX3 (at 0 -1.509) (layer F.Fab) hide)
    (fp_text user gge134453 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.016 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at 0.102 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 3 smd rect (at 1.219 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -864.286 -648.627)
    (attr smd)
    (fp_text reference g (at 1.105 -0.132) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134398 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -867.668 -648.627)
    (attr smd)
    (fp_text reference f (at 1.147 -0.025) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134382 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -871.051 -648.627)
    (attr smd)
    (fp_text reference e (at 1.126 -0.056) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134366 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -878.908 -648.627)
    (attr smd)
    (fp_text reference c (at 1.109 -0.119) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134350 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -882.29 -648.627)
    (attr smd)
    (fp_text reference b (at 1.139 0.013) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134334 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
  )
  (module easyeda:JUMPER_PADSX2 (layer F.Cu) (tedit 0)
    (at -885.673 -648.627)
    (attr smd)
    (fp_text reference a (at 1.105 -0.005) (layer F.SilkS))
    (fp_text value JUMPER_PADSX2 (at -0.508 -1.534) (layer F.Fab) hide)
    (fp_text user gge134318 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0.229 0 90) (size 1.27 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
  )
  (module easyeda:JUMPER (layer F.Cu) (tedit 0)
    (at -871.499 -657.542)
    (attr smd)
    (fp_text reference 1 (at -1.93 -1.991) (layer F.SilkS))
    (fp_text value 3 (at 1.727 -1.991) (layer F.SilkS))
    (fp_text user gge132482 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.829 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at -1.829 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 1 smd rect (at 0.025 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at 0.025 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 1 smd rect (at 1.88 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at 1.88 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
  )
  (module easyeda:JUMPER (layer F.Cu) (tedit 0)
    (at -884.72 -657.568)
    (attr smd)
    (fp_text reference 1 (at -2.019 -1.991) (layer F.SilkS))
    (fp_text value 3 (at 1.727 -1.991) (layer F.SilkS))
    (fp_text user gge132440 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.829 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at -1.829 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 1 smd rect (at 0.025 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0.025 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 1 smd rect (at 1.88 0 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 1.88 -0.864 90) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
  )
  (module easyeda:0805 (layer F.Cu) (tedit 0)
    (at -864.667 -654.71 180)
    (attr smd)
    (fp_text reference C9 (at -0.41 0.131 90) (layer F.SilkS))
    (fp_text value 0805 (at 0.762 -2.245 180) (layer F.Fab) hide)
    (fp_text user gge124077 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.94 -1.016 90) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at 0.94 1.143 90) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
  )
  (module easyeda:0805 (layer F.Cu) (tedit 0)
    (at -885.698 -654.71 180)
    (attr smd)
    (fp_text reference C16 (at -0.321 0.278 90) (layer F.SilkS))
    (fp_text value 0805 (at 0.762 -2.245 180) (layer F.Fab) hide)
    (fp_text user gge124040 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.94 -1.016 90) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0.94 1.143 90) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
  )
  (module easyeda:JUMPER_SOLDER_1X2 (layer F.Cu) (tedit 0)
    (at -861.06 -681.279)
    (attr smd)
    (fp_text reference JP1 (at 3.277 -1.181) (layer Cmts.User))
    (fp_text value JUMPER_SOLDER_1X2 (at 0 -1.712) (layer F.Fab) hide)
    (fp_text user gge110185 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.66 0 90) (size 1.422 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.66 0 90) (size 1.422 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 LPF))
  )
  (module easyeda:CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (layer F.Cu) (tedit 0)
    (at -883.59 -673.735 90)
    (attr smd)
    (fp_text reference C22 (at -1.958 -3.645) (layer F.SilkS))
    (fp_text value CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (at -0.254 -2.372 90) (layer F.Fab) hide)
    (fp_text user gge36226 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.524 0 90) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 SR))
    (pad 2 smd rect (at 1.527 0 90) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 SR))
  )
  (module easyeda:TSSOP-14 (layer F.Cu) (tedit 0)
    (at -862.2 -672.2)
    (attr smd)
    (fp_text reference U2 (at -0.508 -0.65) (layer F.SilkS))
    (fp_text value THS7374IPWR (at -4.605 3.924 90) (layer Cmts.User) hide)
    (fp_text user rep24 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.905 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at -1.255 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
    (pad 3 smd rect (at -0.605 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
    (pad 4 smd rect (at 0.046 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
    (pad 5 smd rect (at 0.695 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.344 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 1.994 2.413 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "NET-(U101-PAD7)"))
    (pad 8 smd rect (at 1.994 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "NET-(U101-PAD8)"))
    (pad 9 smd rect (at 1.344 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 LPF))
    (pad 10 smd rect (at 0.695 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 11 smd rect (at 0.046 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 B-OUT))
    (pad 12 smd rect (at -0.605 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 G-OUT))
    (pad 13 smd rect (at -1.255 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 R-OUT))
    (pad 14 smd rect (at -1.905 -3.588 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -860.488 -663.27)
    (attr smd)
    (fp_text reference R9 (at -0.302 1.618 90) (layer F.SilkS))
    (fp_text value 1.00k (at -2.096 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep30 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.444 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.444 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -859.231 -654.253 90)
    (attr smd)
    (fp_text reference B1 (at -0.203 -2.286 90) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -1.27 -4.139 90) (layer Cmts.User) hide)
    (fp_text user rep34 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.508 -0.889 90) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -871.318 -653.9)
    (attr smd)
    (fp_text reference C11 (at 0.189 2.807 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -3.429 4.959 90) (layer Cmts.User) hide)
    (fp_text user rep59 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
    (pad 2 smd rect (at -0.889 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -868.867 -648.566 180)
    (attr smd)
    (fp_text reference C10 (at -1.764 2.47 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -3.175 4.959 -90) (layer Cmts.User) hide)
    (fp_text user rep65 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.635 3.617 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
    (pad 2 smd rect (at -0.635 1.717 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -874.08 -652.346 180)
    (attr smd)
    (fp_text reference C12 (at -0.272 2.54 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -1.651 4.959 -90) (layer Cmts.User) hide)
    (fp_text user rep71 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.889 3.617 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at 0.889 1.717 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -877.784 -652.346 180)
    (attr smd)
    (fp_text reference C13 (at -1.677 2.54 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -3.048 4.959 -90) (layer Cmts.User) hide)
    (fp_text user rep77 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.508 3.617 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at -0.508 1.717 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -880.916 -648.569 180)
    (attr smd)
    (fp_text reference C14 (at -1.788 2.438 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -3.302 4.959 -90) (layer Cmts.User) hide)
    (fp_text user rep83 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.762 3.617 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
    (pad 2 smd rect (at -0.762 1.717 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -883.11 -653.9)
    (attr smd)
    (fp_text reference C15 (at 0.056 2.837 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at -3.556 4.959 90) (layer Cmts.User) hide)
    (fp_text user rep89 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.016 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
    (pad 2 smd rect (at -1.016 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -870.928 -663.664 270)
    (attr smd)
    (fp_text reference C18 (at -1.509 -1.298 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -5.251 -2.731 270) (layer Cmts.User) hide)
    (fp_text user rep107 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -3.109 -0.191 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
    (pad 2 smd rect (at -1.209 -0.191 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -885.088 -668.109)
    (attr smd)
    (fp_text reference C19 (at -1.966 2.007 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -3.429 4.489 90) (layer Cmts.User) hide)
    (fp_text user rep113 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 2.347 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
    (pad 2 smd rect (at -0.889 0.447 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:1206_P (layer F.Cu) (tedit 0)
    (at -865.975 -667.893 90)
    (attr smd)
    (fp_text reference C7 (at 2.385 -6.084) (layer F.SilkS))
    (fp_text value 22uF/10V (at 4.47 0.216 180) (layer Cmts.User) hide)
    (fp_text user rep146 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.27 -3.429) (size 1.6 1.798) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.27 -0.629) (size 1.6 1.798) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -859.231 -651.689 90)
    (attr smd)
    (fp_text reference G1 (at 0.178 -2.286 90) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -0.889 -4.139 90) (layer Cmts.User) hide)
    (fp_text user rep162 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.888 -0.889 90) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -859.231 -651.662 90)
    (attr smd)
    (fp_text reference R1 (at -1.981 -2.286 90) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -3.048 -4.139 90) (layer Cmts.User) hide)
    (fp_text user rep179 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.27 -0.889 90) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -867.575 -662.038)
    (attr smd)
    (fp_text reference R1 (at 0.076 5.016 90) (layer F.SilkS))
    (fp_text value 2.20k (at -2.54 4.159 90) (layer Cmts.User) hide)
    (fp_text user rep185 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at 0 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -863.295 -655.79 180)
    (attr smd)
    (fp_text reference R3 (at 1.196 2.277 90) (layer F.SilkS))
    (fp_text value 5.62k (at 2.794 5.175 -90) (layer Cmts.User) hide)
    (fp_text user rep191 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
    (pad 2 smd rect (at 0.254 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -862.486 -655.79 180)
    (attr smd)
    (fp_text reference R4 (at -0.039 2.402 90) (layer F.SilkS))
    (fp_text value 5.62k (at 1.651 5.175 -90) (layer Cmts.User) hide)
    (fp_text user rep197 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
    (pad 2 smd rect (at -0.889 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -859.134 -655.79 180)
    (attr smd)
    (fp_text reference R5 (at 1.395 2.279 90) (layer F.SilkS))
    (fp_text value 5.62k (at 3.047 5.175 -90) (layer Cmts.User) hide)
    (fp_text user rep203 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.507 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
    (pad 2 smd rect (at 0.507 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -866.647 -655.79 180)
    (attr smd)
    (fp_text reference R2 (at -0.225 2.355 90) (layer F.SilkS))
    (fp_text value 5.62k (at 1.397 5.175 -90) (layer Cmts.User) hide)
    (fp_text user rep209 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.143 1.717 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at -1.143 3.617 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -863.354 -663.27)
    (attr smd)
    (fp_text reference R7 (at -1.501 1.482 90) (layer F.SilkS))
    (fp_text value 1.00k (at -3.175 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep215 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.635 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -863.161 -663.27)
    (attr smd)
    (fp_text reference R8 (at 0.109 1.52 90) (layer F.SilkS))
    (fp_text value 1.00k (at -1.397 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep221 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.143 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.143 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -865.962 -663.27)
    (attr smd)
    (fp_text reference R6 (at -0.835 1.39 90) (layer F.SilkS))
    (fp_text value 1.00k (at -2.54 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep227 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -864.006 -651.36)
    (attr smd)
    (fp_text reference R12 (at 1.045 0.358 90) (layer F.SilkS))
    (fp_text value 2.20k (at -2.794 1.619 90) (layer Cmts.User) hide)
    (fp_text user rep245 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.254 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at -0.254 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -870.475 -651.36)
    (attr smd)
    (fp_text reference R14 (at 1.365 0.259 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.286 1.219 90) (layer Cmts.User) hide)
    (fp_text user rep251 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
    (pad 2 smd rect (at 0.254 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -866.753 -651.36)
    (attr smd)
    (fp_text reference R13 (at 1.53 0.307 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.032 1.219 90) (layer Cmts.User) hide)
    (fp_text user rep257 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.508 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
    (pad 2 smd rect (at 0.508 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -878.547 -651.36)
    (attr smd)
    (fp_text reference R17 (at 1.45 0.27 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.159 1.219 90) (layer Cmts.User) hide)
    (fp_text user rep269 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.381 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
    (pad 2 smd rect (at 0.381 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -882.266 -651.36)
    (attr smd)
    (fp_text reference R18 (at 1.232 0.231 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.413 1.219 90) (layer Cmts.User) hide)
    (fp_text user rep275 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.127 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
    (pad 2 smd rect (at 0.127 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -885.594 -651.36)
    (attr smd)
    (fp_text reference R19 (at 0.572 0.215 90) (layer F.SilkS))
    (fp_text value 2.20k (at -2.921 1.619 90) (layer Cmts.User) hide)
    (fp_text user rep281 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.381 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at -0.381 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -870.75 -662.8)
    (attr smd)
    (fp_text reference R28 (at 2.378 1.275 90) (layer F.SilkS))
    (fp_text value 6.19k (at -1.27 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep287 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.27 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at 1.27 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -872.006 -656.153)
    (attr smd)
    (fp_text reference R21 (at 2.796 1.214 90) (layer F.SilkS))
    (fp_text value 130k (at -0.889 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep293 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.651 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
    (pad 2 smd rect (at 1.651 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -867.412 -656.153)
    (attr smd)
    (fp_text reference R20 (at 0.433 1.262 90) (layer F.SilkS))
    (fp_text value 130k (at -3.175 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep299 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.635 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
    (pad 2 smd rect (at -0.635 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -873.55 -656.153)
    (attr smd)
    (fp_text reference R22 (at 2.079 1.309 90) (layer F.SilkS))
    (fp_text value 100k (at -1.651 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep305 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.889 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at 0.889 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -879.075 -656.153)
    (attr smd)
    (fp_text reference R23 (at 0.683 1.219 90) (layer F.SilkS))
    (fp_text value 100k (at -3.048 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep311 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.508 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at -0.508 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -882.524 -656.153)
    (attr smd)
    (fp_text reference R24 (at 1.714 1.232 90) (layer F.SilkS))
    (fp_text value 130k (at -1.905 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep317 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.635 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
    (pad 2 smd rect (at 0.635 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -884.451 -656.153)
    (attr smd)
    (fp_text reference R25 (at 1.325 1.237 90) (layer F.SilkS))
    (fp_text value 130k (at -2.286 2.235 90) (layer Cmts.User) hide)
    (fp_text user rep323 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
    (pad 2 smd rect (at 0.254 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -882.713 -662.864)
    (attr smd)
    (fp_text reference R31 (at 1.082 1.224 90) (layer F.SilkS))
    (fp_text value 6.19k (at -2.54 2.635 90) (layer Cmts.User) hide)
    (fp_text user rep329 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -881.05 -658.533 90)
    (attr smd)
    (fp_text reference R27 (at -0.83 0.358 90) (layer F.SilkS))
    (fp_text value 10.0k (at 0.667 -1.524 90) (layer Cmts.User) hide)
    (fp_text user rep335 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.209 1.016 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 3.109 1.016 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 6 S$33979))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -878.726 -662.851 270)
    (attr smd)
    (fp_text reference R26 (at 5.39 -0.473 90) (layer F.SilkS))
    (fp_text value 10.0k (at -0.349 2.159 270) (layer Cmts.User) hide)
    (fp_text user rep341 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 3.109 -0.381 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.209 -0.381 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 6 S$33979))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -871.461 -663.651 270)
    (attr smd)
    (fp_text reference R35 (at -1.392 0.188 90) (layer F.SilkS))
    (fp_text value 162k (at -3.251 -1.334 270) (layer Cmts.User) hide)
    (fp_text user rep347 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -3.109 1.206 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
    (pad 2 smd rect (at -1.209 1.206 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -883.806 -668.122)
    (attr smd)
    (fp_text reference R34 (at -0.835 2.157 90) (layer F.SilkS))
    (fp_text value 162k (at -2.413 2.489 90) (layer Cmts.User) hide)
    (fp_text user rep353 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.127 2.347 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
    (pad 2 smd rect (at 0.127 0.447 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -885.266 -670.636)
    (attr smd)
    (fp_text reference R37 (at -2.07 1.044) (layer F.SilkS))
    (fp_text value 332 (at -0.438 3.556) (layer Cmts.User) hide)
    (fp_text user rep359 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 2.22 1.016 180) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
    (pad 2 smd rect (at 0.32 1.016 180) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 23 SR))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -876.084 -670.636)
    (attr smd)
    (fp_text reference R36 (at -6.109 1.082) (layer F.SilkS))
    (fp_text value 332 (at -3.486 -1.524) (layer Cmts.User) hide)
    (fp_text user rep365 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -3.744 1.016) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 5 SL))
    (pad 2 smd rect (at -1.844 1.016) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -859.231 -649.035 90)
    (attr smd)
    (fp_text reference S1 (at -1.537 -2.286 90) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -2.604 -4.139 90) (layer Cmts.User) hide)
    (fp_text user rep369 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.827 -0.889 90) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -873.379 -645.49)
    (attr smd)
    (fp_text reference SL1 (at 0.076 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -0.635 -4.139) (layer Cmts.User) hide)
    (fp_text user rep373 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.143 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 13 32X-LEFT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -883.285 -645.49)
    (attr smd)
    (fp_text reference SR2 (at -0.623 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -1.397 -4.139) (layer Cmts.User) hide)
    (fp_text user rep377 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.381 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 SCD-RIGHT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -876.554 -645.49)
    (attr smd)
    (fp_text reference SN1 (at -0.305 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -1.016 -4.139) (layer Cmts.User) hide)
    (fp_text user rep381 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.762 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -867.407 -645.49)
    (attr smd)
    (fp_text reference XL1 (at -2.337 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -3.048 -4.139) (layer Cmts.User) hide)
    (fp_text user rep404 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.273 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 SCD-LEFT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -879.856 -645.49)
    (attr smd)
    (fp_text reference XR2 (at -0.496 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -1.27 -4.139) (layer Cmts.User) hide)
    (fp_text user rep408 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.508 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 11 32X-RIGHT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -866.14 -645.49)
    (attr smd)
    (fp_text reference YL1 (at -0.051 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -0.762 -4.139) (layer Cmts.User) hide)
    (fp_text user rep412 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 1.016 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -886.714 -645.49)
    (attr smd)
    (fp_text reference YR2 (at -0.75 -2.286) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -1.524 -4.139) (layer Cmts.User) hide)
    (fp_text user rep416 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 -0.889) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
  )
  (module easyeda:TP50 (layer F.Cu) (tedit 0)
    (at -860.984 -645.008 270)
    (attr smd)
    (fp_text reference 5V1 (at -1.956 -2.286 90) (layer F.SilkS) hide)
    (fp_text value TP_50 (at -2.794 -4.139 270) (layer Cmts.User) hide)
    (fp_text user rep424 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.016 -0.889 270) (size 1.27 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
  )
  (module easyeda:OSHW-LOGO_5MM (layer F.Cu) (tedit 0)
    (at -885.774 -680.644)
    (fp_text reference G (at 0.743 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.293 0) (layer F.Fab) hide)
    (fp_text user rep451 (at 0 0) (layer Cmts.User))
  )
  (module easyeda:1206_P (layer F.Cu) (tedit 0)
    (at -874.687 -659.574 270)
    (attr smd)
    (fp_text reference C17 (at -0.366 0.836) (layer F.SilkS))
    (fp_text value 22uF/10V (at -3.823 -1.803 270) (layer Cmts.User) hide)
    (fp_text user gge1266 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.778 1.397 270) (size 1.6 1.798) (layers F.Cu F.Paste F.Mask)
      (net 6 S$33979))
    (pad 2 smd rect (at 1.022 1.397 270) (size 1.6 1.798) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -864.781 -670.179)
    (attr smd)
    (fp_text reference C6 (at -1.385 -4.087) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 1.778 2.076 90) (layer Cmts.User) hide)
    (fp_text user rep152 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.762 -2.982 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.762 -1.082 270) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -875.906 -668.896 270)
    (attr smd)
    (fp_text reference C20 (at -0.77 1.131) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 1.778 2.076) (layer Cmts.User) hide)
    (fp_text user gge34394 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.762 -2.982 180) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.762 -1.082 180) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -867.232 -675.919 90)
    (attr smd)
    (fp_text reference R11 (at 0.963 0.559) (layer F.SilkS))
    (fp_text value 1.00k (at -2.54 2.635 180) (layer Cmts.User) hide)
    (fp_text user gge35720 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093 180) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at 0 0.193 180) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (layer F.Cu) (tedit 0)
    (at -877.443 -672.478)
    (attr smd)
    (fp_text reference C21 (at -2.603 -2.271) (layer F.SilkS))
    (fp_text value CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (at -0.254 -2.372) (layer F.Fab) hide)
    (fp_text user gge36276 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.524 0) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 SL))
    (pad 2 smd rect (at 1.527 0) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 SL))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -865.111 -666.788)
    (attr smd)
    (fp_text reference C2 (at -0.797 -0.203 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -3.429 4.489 90) (layer Cmts.User) hide)
    (fp_text user gge109221 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 2.347 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at -0.889 0.447 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -864.906 -663.997 180)
    (attr smd)
    (fp_text reference C3 (at -0.903 3.046 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -3.429 4.489 -90) (layer Cmts.User) hide)
    (fp_text user gge109240 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 2.347 270) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
    (pad 2 smd rect (at -0.889 0.447 270) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 20 R-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -861.151 -666.788)
    (attr smd)
    (fp_text reference C4 (at -0.77 -0.124 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -3.429 4.489 90) (layer Cmts.User) hide)
    (fp_text user gge109259 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 2.347 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
    (pad 2 smd rect (at -0.889 0.447 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 21 G-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -859.168 -666.788)
    (attr smd)
    (fp_text reference C5 (at -0.81 -0.229 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at -3.429 4.489 90) (layer Cmts.User) hide)
    (fp_text user gge109632 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.889 2.347 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
    (pad 2 smd rect (at -0.889 0.447 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 22 B-IN))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -859.853 -679.234 270)
    (attr smd)
    (fp_text reference R10 (at -0.162 4.229) (layer F.SilkS))
    (fp_text value 1.00k (at -2.54 2.635) (layer Cmts.User) hide)
    (fp_text user gge111153 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0.193) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 7 LPF))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -884.784 -662.864)
    (attr smd)
    (fp_text reference R32 (at 1.046 1.245 90) (layer F.SilkS))
    (fp_text value 6.19k (at -2.54 2.635 90) (layer Cmts.User) hide)
    (fp_text user gge122953 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -886.79 -662.864)
    (attr smd)
    (fp_text reference R33 (at 1.084 1.236 90) (layer F.SilkS))
    (fp_text value 6.19k (at -2.54 2.635 90) (layer Cmts.User) hide)
    (fp_text user gge122974 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 9 YM-RIGHT))
    (pad 2 smd rect (at 0 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 4 RIGHT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -872.884 -662.8)
    (attr smd)
    (fp_text reference R30 (at 0.411 1.212 90) (layer F.SilkS))
    (fp_text value 130k (at -3.175 2.235 90) (layer Cmts.User) hide)
    (fp_text user gge122995 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.635 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at -0.635 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -870.865 -662.8)
    (attr smd)
    (fp_text reference R29 (at 0.463 1.26 90) (layer F.SilkS))
    (fp_text value 130k (at -3.175 2.235 90) (layer Cmts.User) hide)
    (fp_text user gge123015 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.635 2.093 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 8 YM-LEFT))
    (pad 2 smd rect (at -0.635 0.193 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 15 LEFT))
  )
  (module easyeda:CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (layer F.Cu) (tedit 0)
    (at -870.801 -672.478 180)
    (attr smd)
    (fp_text reference C8 (at 3.924 1.001) (layer F.SilkS))
    (fp_text value CP_TANTALUM_CASE-B_EIA-3528-21_REFLOW (at -0.254 -2.372 180) (layer F.Fab) hide)
    (fp_text user gge125200 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -1.524 0 180) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 SYNC-OUT))
    (pad 2 smd rect (at 1.527 0 180) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 SYNC-75))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -874.446 -651.36)
    (attr smd)
    (fp_text reference R15 (at 1.273 0.257 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.286 1.219 90) (layer Cmts.User) hide)
    (fp_text user gge129590 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at 0.254 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -876.432 -651.36)
    (attr smd)
    (fp_text reference R16 (at 1.316 0.241 90) (layer F.SilkS))
    (fp_text value 75.0 (at -2.286 1.219 90) (layer Cmts.User) hide)
    (fp_text user gge130138 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at 0.254 1.077 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 12 PSG))
    (pad 2 smd rect (at 0.254 -0.823 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module easyeda:0603 (layer F.Cu) (tedit 0)
    (at -868.743 -667.423 180)
    (attr smd)
    (fp_text reference C1 (at -0.841 -0.436 90) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 1.778 2.076 -90) (layer Cmts.User) hide)
    (fp_text user gge131926 (at 0 0) (layer Cmts.User))
    (pad 1 smd rect (at -0.762 -2.982 90) (size 0.8 1.001) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at -0.762 -1.082 90) (size 0.798 1.001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_line (start -858.761 -645.033) (end -887.768 -645.033) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -887.768 -645.033) (end -887.768 -683.565) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -887.768 -683.565) (end -858.749 -683.565) (layer Edge.Cuts) (width 0.254))
  (gr_line (start -858.749 -683.565) (end -858.749 -645.033) (layer Edge.Cuts) (width 0.254))
  (gr_text "Licensed under CERN OHL v.1.2" (at -862.724 -651.307) (layer B.SilkS))
  (gr_text "Jumper settings" (at -869.277 -668.515) (layer B.SilkS))
  (gr_text "Original design by db electronics" (at -862.208 -648.153) (layer B.SilkS))
  (gr_text 5V (at -873.636 -679.414) (layer B.SilkS))
  (gr_text SR (at -876.905 -676.735) (layer B.SilkS))
  (gr_text SL (at -875.017 -676.798) (layer B.SilkS))
  (gr_text 75 (at -870.859 -676.697) (layer B.SilkS))
  (gr_text S (at -873.199 -676.773) (layer B.SilkS))
  (gr_text B (at -872.005 -679.465) (layer B.SilkS))
  (gr_text G (at -869.15 -679.541) (layer B.SilkS))
  (gr_text R (at -869.236 -676.697) (layer B.SilkS))
  (gr_text "M1va0-6.5= 1\nM1va7 & M2va0-1.8= 2, c, d-right, e\nM2Va3= 2\nM2va2-2.3= 1, d-left\nM2va4= 3, d-right\nM3va1/2= 3, b, c, d-right, e, f" (at -860.26 -667.398) (layer B.SilkS))
  (gr_text "MDFourier POWERED" (at -867.619 -670.314) (layer B.SilkS))
  (gr_text Cruzlink2 (at -862.838 -654.482) (layer B.SilkS))
  (gr_text RetroRGB (at -862.838 -655.904) (layer B.SilkS))
  (gr_text Artemio (at -862.838 -653.06) (layer B.SilkS))
  (gr_text Ace (at -876.554 -656.107) (layer B.SilkS))
  (gr_text "Firebrand X" (at -876.554 -653.351) (layer B.SilkS))
  (gr_text Mobiusstriptech (at -876.554 -654.871) (layer B.SilkS))
  (gr_text "Board design by" (at -865.67 -649.719) (layer B.SilkS))
  (gr_text "Special thanks to Bfbiii" (at -866.516 -646.425) (layer B.SilkS))
  (gr_text YR (at -885.025 -645.447 90) (layer F.SilkS))
  (gr_text CR (at -881.444 -645.447 90) (layer F.SilkS))
  (gr_text XR (at -877.862 -645.447 90) (layer F.SilkS))
  (gr_text PSG (at -874.281 -645.447 90) (layer F.SilkS))
  (gr_text CL (at -867.118 -645.447 90) (layer F.SilkS))
  (gr_text XL (at -870.7 -645.447 90) (layer F.SilkS))
  (gr_text 5V (at -861.784 -645.51 90) (layer F.SilkS))
  (gr_text B (at -861.733 -654.573 90) (layer F.SilkS))
  (gr_text G (at -861.695 -652.378 90) (layer F.SilkS))
  (gr_text R (at -861.67 -650.217 90) (layer F.SilkS))
  (gr_text GND (at -887.362 -676.488) (layer F.SilkS))
  (gr_text LPF (at -861.797 -682.869) (layer F.SilkS))
  (gr_text S (at -861.733 -647.982 90) (layer F.SilkS))
  (gr_text YL (at -863.536 -645.447 90) (layer F.SilkS))
  (gr_text 5V (at -874.852 -679.427) (layer F.SilkS))
  (gr_text SR (at -878.154 -676.76) (layer F.SilkS))
  (gr_text SL (at -876.046 -676.798) (layer F.SilkS))
  (gr_text 75 (at -872.02 -676.722) (layer F.SilkS))
  (gr_text S (at -873.696 -676.786) (layer F.SilkS))
  (gr_text B (at -872.439 -679.427) (layer F.SilkS))
  (gr_text G (at -869.759 -679.427) (layer F.SilkS))
  (gr_text R (at -869.645 -676.747) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -858.38 -684.085) (xy -858.063 -643.776) (xy -889.305 -643.852) (xy -888.492 -684.263)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -888.898 -644.131) (xy -889.178 -685.241) (xy -858.329 -684.149) (xy -857.936 -644.233)
      )
    )
  )
)
